<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<settings>
<setting alwaysvectorfont="no"/>
<setting verticaltext="up"/>
</settings>
<grid distance="0.05" unitdist="inch" unit="inch" style="lines" multiple="1" display="yes" altdistance="0.005" altunitdist="inch" altunit="inch"/>
<layers>
<layer number="1" name="Top" color="4" fill="1" visible="yes" active="yes"/>
<layer number="16" name="Bottom" color="1" fill="1" visible="yes" active="yes"/>
<layer number="17" name="Pads" color="2" fill="1" visible="yes" active="yes"/>
<layer number="18" name="Vias" color="2" fill="1" visible="yes" active="yes"/>
<layer number="19" name="Unrouted" color="6" fill="1" visible="yes" active="yes"/>
<layer number="20" name="Dimension" color="15" fill="1" visible="yes" active="yes"/>
<layer number="21" name="tPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="22" name="bPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="23" name="tOrigins" color="15" fill="1" visible="yes" active="yes"/>
<layer number="24" name="bOrigins" color="15" fill="1" visible="yes" active="yes"/>
<layer number="25" name="tNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="26" name="bNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="27" name="tValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="28" name="bValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="29" name="tStop" color="7" fill="3" visible="no" active="yes"/>
<layer number="30" name="bStop" color="7" fill="6" visible="no" active="yes"/>
<layer number="31" name="tCream" color="7" fill="4" visible="no" active="yes"/>
<layer number="32" name="bCream" color="7" fill="5" visible="no" active="yes"/>
<layer number="33" name="tFinish" color="6" fill="3" visible="no" active="yes"/>
<layer number="34" name="bFinish" color="6" fill="6" visible="no" active="yes"/>
<layer number="35" name="tGlue" color="7" fill="4" visible="no" active="yes"/>
<layer number="36" name="bGlue" color="7" fill="5" visible="no" active="yes"/>
<layer number="37" name="tTest" color="7" fill="1" visible="no" active="yes"/>
<layer number="38" name="bTest" color="7" fill="1" visible="no" active="yes"/>
<layer number="39" name="tKeepout" color="4" fill="11" visible="yes" active="yes"/>
<layer number="40" name="bKeepout" color="1" fill="11" visible="yes" active="yes"/>
<layer number="41" name="tRestrict" color="4" fill="10" visible="yes" active="yes"/>
<layer number="42" name="bRestrict" color="1" fill="10" visible="yes" active="yes"/>
<layer number="43" name="vRestrict" color="2" fill="10" visible="yes" active="yes"/>
<layer number="44" name="Drills" color="7" fill="1" visible="no" active="yes"/>
<layer number="45" name="Holes" color="7" fill="1" visible="no" active="yes"/>
<layer number="46" name="Milling" color="3" fill="1" visible="no" active="yes"/>
<layer number="47" name="Measures" color="7" fill="1" visible="no" active="yes"/>
<layer number="48" name="Document" color="7" fill="1" visible="yes" active="yes"/>
<layer number="49" name="Reference" color="7" fill="1" visible="yes" active="yes"/>
<layer number="51" name="tDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="52" name="bDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="91" name="Nets" color="2" fill="1" visible="yes" active="yes"/>
<layer number="92" name="Busses" color="1" fill="1" visible="yes" active="yes"/>
<layer number="93" name="Pins" color="2" fill="1" visible="yes" active="yes"/>
<layer number="94" name="Symbols" color="4" fill="1" visible="yes" active="yes"/>
<layer number="95" name="Names" color="7" fill="1" visible="yes" active="yes"/>
<layer number="96" name="Values" color="7" fill="1" visible="yes" active="yes"/>
<layer number="97" name="Info" color="7" fill="1" visible="yes" active="yes"/>
<layer number="98" name="Guide" color="6" fill="1" visible="yes" active="yes"/>
</layers>
<library>
<description>2.4GHz Transceiver from Nordic Semiconductors</description>
<packages>
<package name="NRF24L01_MODULE_FOOTPRINT">
<description>This module based on Nordic nRF24L01, highly integrated, ultra low power (ULP) 2Mbps RF transceiver for the 2.4GHz ISM (Industrial, Scientific and Medical) band.  
Nordic nRF24L01+ integrates a complete 2.4GHz RF transceiver, RF synthesizer, and baseband logic including the Enhanced ShockBurst™ hardware protocol accelerator 
supporting a high-speed SPI interface for the application controller.</description>
<pad name="CE" x="-13.97" y="3.81" drill="0.9" diameter="1.778"/>
<pad name="CSN" x="-11.43" y="3.81" drill="0.9" diameter="1.778"/>
<pad name="GND" x="-13.97" y="6.35" drill="0.9" diameter="1.778" shape="square"/>
<pad name="3_3_V" x="-11.43" y="6.35" drill="0.9" diameter="1.778"/>
<pad name="SCLK" x="-13.97" y="1.27" drill="0.9" diameter="1.778"/>
<pad name="MOSI" x="-11.43" y="1.27" drill="0.9" diameter="1.778"/>
<pad name="MISO" x="-13.97" y="-1.27" drill="0.9" diameter="1.778"/>
<pad name="IRQ" x="-11.43" y="-1.27" drill="0.9" diameter="1.778"/>
<wire x1="-15.24" y1="7.62" x2="-15.24" y2="-7.62" width="0.127" layer="21"/>
<wire x1="-15.24" y1="-7.62" x2="15.24" y2="-7.62" width="0.127" layer="21"/>
<wire x1="15.24" y1="-7.62" x2="15.24" y2="7.62" width="0.127" layer="21"/>
<wire x1="15.24" y1="7.62" x2="-15.24" y2="7.62" width="0.127" layer="21"/>
<text x="-17.018" y="6.096" size="0.6096" layer="21">GND</text>
<text x="-16.51" y="3.556" size="0.6096" layer="21">CE</text>
<text x="-17.526" y="1.016" size="0.6096" layer="21">SCLK</text>
<text x="-17.399" y="-1.524" size="0.6096" layer="21">MISO</text>
<text x="-10.16" y="6.096" size="0.6096" layer="21">3.3V</text>
<text x="-10.16" y="3.556" size="0.6096" layer="21">CSN</text>
<text x="-10.16" y="1.016" size="0.6096" layer="21">MOSI</text>
<text x="-10.16" y="-1.524" size="0.6096" layer="21">IRQ</text>
<text x="-15.24" y="8.255" size="1.016" layer="25" ratio="12">&gt;NAME</text>
</package>
<package name="MC1320X_AND_NRF24L01_FOOTPRINT">
<description>With this Footprint, it is possible to use the NRF24L01 or the MC1320x 802.15.4 transceiver</description>
<pad name="CE" x="-13.97" y="3.81" drill="0.9" diameter="1.4224"/>
<pad name="CSN" x="-11.43" y="3.81" drill="0.9" diameter="1.4224"/>
<pad name="GND" x="-13.97" y="6.35" drill="0.9" diameter="1.4224" shape="square"/>
<pad name="3_3_V" x="-11.43" y="6.35" drill="0.9" diameter="1.4224"/>
<pad name="SCLK" x="-13.97" y="1.27" drill="0.9" diameter="1.4224"/>
<pad name="MOSI" x="-11.43" y="1.27" drill="0.9" diameter="1.4224"/>
<pad name="MISO" x="-13.97" y="-1.27" drill="0.9" diameter="1.4224"/>
<pad name="IRQ" x="-11.43" y="-1.27" drill="0.9" diameter="1.4224"/>
<wire x1="-15.24" y1="7.62" x2="-15.24" y2="-6.985" width="0.127" layer="21"/>
<wire x1="-15.24" y1="-6.985" x2="12.7" y2="-6.985" width="0.127" layer="21"/>
<wire x1="12.7" y1="-6.985" x2="12.7" y2="7.62" width="0.127" layer="21"/>
<wire x1="12.7" y1="7.62" x2="-15.24" y2="7.62" width="0.127" layer="21"/>
<text x="-17.018" y="6.096" size="0.6096" layer="21">GND</text>
<text x="-16.51" y="3.556" size="0.6096" layer="21">CE</text>
<text x="-17.526" y="1.016" size="0.6096" layer="21">SCLK</text>
<text x="-17.399" y="-1.524" size="0.6096" layer="21">MISO</text>
<text x="-10.16" y="6.096" size="0.6096" layer="21">3.3V</text>
<text x="-10.16" y="3.556" size="0.6096" layer="21">CSN</text>
<text x="-10.16" y="1.016" size="0.6096" layer="21">MOSI</text>
<text x="-10.16" y="-1.524" size="0.6096" layer="21">IRQ</text>
<text x="-15.24" y="8.255" size="1.016" layer="21" ratio="12">&gt;NAME</text>
<pad name="GND1" x="-2.54" y="6.35" drill="0.9" diameter="1.4224" shape="square"/>
<pad name="SS" x="0" y="6.35" drill="0.9" diameter="1.4224"/>
<pad name="3_3_V1" x="-2.54" y="3.81" drill="0.9" diameter="1.4224"/>
<pad name="RXTXEN" x="0" y="3.81" drill="0.9" diameter="1.4224"/>
<pad name="SPICLK" x="-2.54" y="1.27" drill="0.9" diameter="1.4224"/>
<pad name="ATTN" x="0" y="1.27" drill="0.9" diameter="1.4224"/>
<pad name="MOSI2" x="-2.54" y="-1.27" drill="0.9" diameter="1.4224"/>
<pad name="RESET" x="0" y="-1.27" drill="0.9" diameter="1.4224"/>
<pad name="MISO2" x="-2.54" y="-3.81" drill="0.9" diameter="1.4224"/>
<pad name="IRQ2" x="0" y="-3.81" drill="0.9" diameter="1.4224"/>
<text x="-5.588" y="6.096" size="0.6096" layer="21">GND</text>
<text x="-5.715" y="3.556" size="0.6096" layer="21">3.3V</text>
<text x="-6.985" y="1.016" size="0.6096" layer="21">SPICLK</text>
<text x="-5.715" y="-1.524" size="0.6096" layer="21">MOSI</text>
<text x="-5.715" y="-4.064" size="0.6096" layer="21">MISO</text>
<text x="1.397" y="6.096" size="0.6096" layer="21">SS</text>
<text x="1.397" y="3.556" size="0.6096" layer="21">RXTXEN</text>
<text x="1.397" y="1.016" size="0.6096" layer="21">ATTN</text>
<text x="1.397" y="-1.524" size="0.6096" layer="21">RESET</text>
<text x="1.397" y="-4.064" size="0.6096" layer="21">IRQ</text>
<text x="-4.318" y="-6.35" size="1.016" layer="21">MC1320X</text>
<text x="-15.113" y="-3.81" size="1.016" layer="21">NRF24L01</text>
</package>
<package name="NRF24L01_MODULE_FOOTPRINT_SMALL">
<pad name="CE" x="-1.27" y="1.27" drill="0.9" diameter="1.6764"/>
<pad name="CSN" x="1.27" y="1.27" drill="0.9" diameter="1.6764"/>
<pad name="GND" x="-1.27" y="3.81" drill="0.9" diameter="1.6764" shape="square"/>
<pad name="3_3_V" x="1.27" y="3.81" drill="0.9" diameter="1.6764"/>
<pad name="SCLK" x="-1.27" y="-1.27" drill="0.9" diameter="1.6764"/>
<pad name="MOSI" x="1.27" y="-1.27" drill="0.9" diameter="1.6764"/>
<pad name="MISO" x="-1.27" y="-3.81" drill="0.9" diameter="1.6764"/>
<pad name="IRQ" x="1.27" y="-3.81" drill="0.9" diameter="1.6764"/>
<wire x1="-2.54" y1="5.08" x2="-2.54" y2="-5.08" width="0.127" layer="21"/>
<wire x1="-2.54" y1="-5.08" x2="2.54" y2="-5.08" width="0.127" layer="21"/>
<wire x1="2.54" y1="-5.08" x2="2.54" y2="5.08" width="0.127" layer="21"/>
<wire x1="2.54" y1="5.08" x2="-2.54" y2="5.08" width="0.127" layer="21"/>
<text x="-2.667" y="3.937" size="0.4064" layer="21" font="vector" rot="R180">GND</text>
<text x="-2.667" y="1.524" size="0.4064" layer="21" font="vector" rot="R180">CE</text>
<text x="-2.667" y="-1.016" size="0.4064" layer="21" font="vector" rot="R180">SCLK</text>
<text x="-2.54" y="-3.556" size="0.4064" layer="21" font="vector" rot="R180">MISO</text>
<text x="2.667" y="3.683" size="0.4064" layer="21" font="vector">3.3V</text>
<text x="2.667" y="1.143" size="0.4064" layer="21" font="vector">CSN</text>
<text x="2.667" y="-1.397" size="0.4064" layer="21" font="vector">MOSI</text>
<text x="2.667" y="-3.937" size="0.4064" layer="21" font="vector">IRQ</text>
<text x="-2.54" y="5.207" size="0.8128" layer="25" font="vector" ratio="12">&gt;NAME</text>
</package>
</packages>
<symbols>
<symbol name="NRF24L01_MODULE_SCHEMATIC">
<description>This module based on Nordic nRF24L01, highly integrated, ultra low power (ULP) 2Mbps RF transceiver for the 2.4GHz ISM (Industrial, Scientific and Medical) band.  
Nordic nRF24L01+ integrates a complete 2.4GHz RF transceiver, RF synthesizer, and baseband logic including the Enhanced ShockBurst™ hardware protocol accelerator 
supporting a high-speed SPI interface for the application controller.</description>
<pin name="GND" x="-15.24" y="7.62" length="middle"/>
<pin name="CE" x="-15.24" y="2.54" length="middle"/>
<pin name="SCK" x="-15.24" y="-2.54" length="middle"/>
<pin name="MISO" x="-15.24" y="-7.62" length="middle"/>
<pin name="3.3V" x="15.24" y="7.62" length="middle" rot="R180"/>
<pin name="CSN" x="15.24" y="2.54" length="middle" rot="R180"/>
<pin name="MOSI" x="15.24" y="-2.54" length="middle" rot="R180"/>
<pin name="IRQ" x="15.24" y="-7.62" length="middle" rot="R180"/>
<wire x1="-10.16" y1="10.16" x2="-10.16" y2="-10.16" width="0.254" layer="94"/>
<wire x1="-10.16" y1="-10.16" x2="10.16" y2="-10.16" width="0.254" layer="94"/>
<wire x1="10.16" y1="-10.16" x2="10.16" y2="10.16" width="0.254" layer="94"/>
<wire x1="10.16" y1="10.16" x2="-10.16" y2="10.16" width="0.254" layer="94"/>
<text x="-10.16" y="10.922" size="1.778" layer="95" ratio="12">&gt;NAME</text>
<text x="-10.16" y="-12.7" size="1.778" layer="96" ratio="12">&gt;VALUE</text>
</symbol>
<symbol name="MC1320X_RF_DAUGHTER_CARD">
<description>The MC1320x RF Daughter Card (1320xRFD-A00) is used in conjunction with a microcontroller development board for RFIC evaluation, code development, and system evaluation.</description>
<pin name="GND" x="-17.78" y="10.16" length="middle"/>
<pin name="3.3V" x="-17.78" y="5.08" length="middle"/>
<pin name="SPICLK" x="-17.78" y="0" length="middle"/>
<pin name="MOSI" x="-17.78" y="-5.08" length="middle"/>
<pin name="MISO" x="-17.78" y="-10.16" length="middle"/>
<pin name="SS" x="15.24" y="10.16" length="middle" rot="R180"/>
<pin name="RXTXEN" x="15.24" y="5.08" length="middle" rot="R180"/>
<pin name="ATTN" x="15.24" y="0" length="middle" rot="R180"/>
<pin name="RESET" x="15.24" y="-5.08" length="middle" rot="R180"/>
<pin name="IRQ" x="15.24" y="-10.16" length="middle" rot="R180"/>
<wire x1="-12.7" y1="12.7" x2="-12.7" y2="-12.7" width="0.254" layer="94"/>
<wire x1="-12.7" y1="-12.7" x2="10.16" y2="-12.7" width="0.254" layer="94"/>
<wire x1="10.16" y1="-12.7" x2="10.16" y2="12.7" width="0.254" layer="94"/>
<wire x1="10.16" y1="12.7" x2="-12.7" y2="12.7" width="0.254" layer="94"/>
<text x="-12.7" y="13.462" size="1.778" layer="94" ratio="12">&gt;NAME</text>
</symbol>
</symbols>
<devicesets>
<deviceset name="NRF24L01_MODULE" prefix="J_NRF24L01_MODULE_">
<description>This module based on Nordic nRF24L01, highly integrated, ultra low power (ULP) 2Mbps RF transceiver for the 2.4GHz ISM (Industrial, Scientific and Medical) band.  
Nordic nRF24L01+ integrates a complete 2.4GHz RF transceiver, RF synthesizer, and baseband logic including the Enhanced ShockBurst™ hardware protocol accelerator 
supporting a high-speed SPI interface for the application controller.</description>
<gates>
<gate name="J_NRF24L01_MODULE" symbol="NRF24L01_MODULE_SCHEMATIC" x="0" y="0"/>
</gates>
<devices>
<device name="" package="NRF24L01_MODULE_FOOTPRINT">
<connects>
<connect gate="J_NRF24L01_MODULE" pin="3.3V" pad="3_3_V"/>
<connect gate="J_NRF24L01_MODULE" pin="CE" pad="CE"/>
<connect gate="J_NRF24L01_MODULE" pin="CSN" pad="CSN"/>
<connect gate="J_NRF24L01_MODULE" pin="GND" pad="GND"/>
<connect gate="J_NRF24L01_MODULE" pin="IRQ" pad="IRQ"/>
<connect gate="J_NRF24L01_MODULE" pin="MISO" pad="MISO"/>
<connect gate="J_NRF24L01_MODULE" pin="MOSI" pad="MOSI"/>
<connect gate="J_NRF24L01_MODULE" pin="SCK" pad="SCLK"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMALL" package="NRF24L01_MODULE_FOOTPRINT_SMALL">
<connects>
<connect gate="J_NRF24L01_MODULE" pin="3.3V" pad="3_3_V"/>
<connect gate="J_NRF24L01_MODULE" pin="CE" pad="CE"/>
<connect gate="J_NRF24L01_MODULE" pin="CSN" pad="CSN"/>
<connect gate="J_NRF24L01_MODULE" pin="GND" pad="GND"/>
<connect gate="J_NRF24L01_MODULE" pin="IRQ" pad="IRQ"/>
<connect gate="J_NRF24L01_MODULE" pin="MISO" pad="MISO"/>
<connect gate="J_NRF24L01_MODULE" pin="MOSI" pad="MOSI"/>
<connect gate="J_NRF24L01_MODULE" pin="SCK" pad="SCLK"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC1320X_AND_NRF24L01" prefix="J_802.15.4_TRANS_">
<description>With this Device, it is possible to use the NRF24L01 or the MC1320x 802.15.4 transceiver</description>
<gates>
<gate name="_MC1320X" symbol="MC1320X_RF_DAUGHTER_CARD" x="2.54" y="-17.78"/>
<gate name="_NRF24L01" symbol="NRF24L01_MODULE_SCHEMATIC" x="0" y="12.7"/>
</gates>
<devices>
<device name="" package="MC1320X_AND_NRF24L01_FOOTPRINT">
<connects>
<connect gate="_MC1320X" pin="3.3V" pad="3_3_V1"/>
<connect gate="_MC1320X" pin="ATTN" pad="ATTN"/>
<connect gate="_MC1320X" pin="GND" pad="GND1"/>
<connect gate="_MC1320X" pin="IRQ" pad="IRQ2"/>
<connect gate="_MC1320X" pin="MISO" pad="MISO2"/>
<connect gate="_MC1320X" pin="MOSI" pad="MOSI2"/>
<connect gate="_MC1320X" pin="RESET" pad="RESET"/>
<connect gate="_MC1320X" pin="RXTXEN" pad="RXTXEN"/>
<connect gate="_MC1320X" pin="SPICLK" pad="SPICLK"/>
<connect gate="_MC1320X" pin="SS" pad="SS"/>
<connect gate="_NRF24L01" pin="3.3V" pad="3_3_V"/>
<connect gate="_NRF24L01" pin="CE" pad="CE"/>
<connect gate="_NRF24L01" pin="CSN" pad="CSN"/>
<connect gate="_NRF24L01" pin="GND" pad="GND"/>
<connect gate="_NRF24L01" pin="IRQ" pad="IRQ"/>
<connect gate="_NRF24L01" pin="MISO" pad="MISO"/>
<connect gate="_NRF24L01" pin="MOSI" pad="MOSI"/>
<connect gate="_NRF24L01" pin="SCK" pad="SCLK"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
