<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<settings>
<setting alwaysvectorfont="no"/>
<setting verticaltext="up"/>
</settings>
<grid distance="0.05" unitdist="inch" unit="inch" style="lines" multiple="1" display="yes" altdistance="0.025" altunitdist="inch" altunit="inch"/>
<layers>
<layer number="1" name="Top" color="4" fill="1" visible="yes" active="yes"/>
<layer number="2" name="Route2" color="1" fill="3" visible="no" active="yes"/>
<layer number="3" name="Route3" color="4" fill="3" visible="no" active="yes"/>
<layer number="4" name="Route4" color="1" fill="4" visible="no" active="yes"/>
<layer number="5" name="Route5" color="4" fill="4" visible="no" active="yes"/>
<layer number="6" name="Route6" color="1" fill="8" visible="no" active="yes"/>
<layer number="7" name="Route7" color="4" fill="8" visible="no" active="yes"/>
<layer number="8" name="Route8" color="1" fill="2" visible="no" active="yes"/>
<layer number="9" name="Route9" color="4" fill="2" visible="no" active="yes"/>
<layer number="10" name="Route10" color="1" fill="7" visible="no" active="yes"/>
<layer number="11" name="Route11" color="4" fill="7" visible="no" active="yes"/>
<layer number="12" name="Route12" color="1" fill="5" visible="no" active="yes"/>
<layer number="13" name="Route13" color="4" fill="5" visible="no" active="yes"/>
<layer number="14" name="Route14" color="1" fill="6" visible="no" active="yes"/>
<layer number="15" name="Route15" color="4" fill="6" visible="no" active="yes"/>
<layer number="16" name="Bottom" color="1" fill="1" visible="yes" active="yes"/>
<layer number="17" name="Pads" color="2" fill="1" visible="yes" active="yes"/>
<layer number="18" name="Vias" color="2" fill="1" visible="yes" active="yes"/>
<layer number="19" name="Unrouted" color="6" fill="1" visible="yes" active="yes"/>
<layer number="20" name="Dimension" color="15" fill="1" visible="yes" active="yes"/>
<layer number="21" name="tPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="22" name="bPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="23" name="tOrigins" color="15" fill="1" visible="yes" active="yes"/>
<layer number="24" name="bOrigins" color="15" fill="1" visible="yes" active="yes"/>
<layer number="25" name="tNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="26" name="bNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="27" name="tValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="28" name="bValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="29" name="tStop" color="7" fill="3" visible="no" active="yes"/>
<layer number="30" name="bStop" color="7" fill="6" visible="no" active="yes"/>
<layer number="31" name="tCream" color="7" fill="4" visible="no" active="yes"/>
<layer number="32" name="bCream" color="7" fill="5" visible="no" active="yes"/>
<layer number="33" name="tFinish" color="6" fill="3" visible="no" active="yes"/>
<layer number="34" name="bFinish" color="6" fill="6" visible="no" active="yes"/>
<layer number="35" name="tGlue" color="7" fill="4" visible="no" active="yes"/>
<layer number="36" name="bGlue" color="7" fill="5" visible="no" active="yes"/>
<layer number="37" name="tTest" color="7" fill="1" visible="no" active="yes"/>
<layer number="38" name="bTest" color="7" fill="1" visible="no" active="yes"/>
<layer number="39" name="tKeepout" color="4" fill="11" visible="yes" active="yes"/>
<layer number="40" name="bKeepout" color="1" fill="11" visible="yes" active="yes"/>
<layer number="41" name="tRestrict" color="4" fill="10" visible="yes" active="yes"/>
<layer number="42" name="bRestrict" color="1" fill="10" visible="yes" active="yes"/>
<layer number="43" name="vRestrict" color="2" fill="10" visible="yes" active="yes"/>
<layer number="44" name="Drills" color="7" fill="1" visible="no" active="yes"/>
<layer number="45" name="Holes" color="7" fill="1" visible="no" active="yes"/>
<layer number="46" name="Milling" color="3" fill="1" visible="no" active="yes"/>
<layer number="47" name="Measures" color="7" fill="1" visible="no" active="yes"/>
<layer number="48" name="Document" color="7" fill="1" visible="yes" active="yes"/>
<layer number="49" name="Reference" color="7" fill="1" visible="yes" active="yes"/>
<layer number="50" name="dxf" color="7" fill="1" visible="yes" active="yes"/>
<layer number="51" name="tDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="52" name="bDocu" color="7" fill="1" visible="yes" active="yes"/>
<layer number="53" name="tGND_GNDA" color="7" fill="9" visible="no" active="no"/>
<layer number="54" name="bGND_GNDA" color="1" fill="9" visible="no" active="no"/>
<layer number="56" name="wert" color="7" fill="1" visible="yes" active="yes"/>
<layer number="91" name="Nets" color="2" fill="1" visible="yes" active="yes"/>
<layer number="92" name="Busses" color="1" fill="1" visible="yes" active="yes"/>
<layer number="93" name="Pins" color="2" fill="1" visible="yes" active="yes"/>
<layer number="94" name="Symbols" color="4" fill="1" visible="yes" active="yes"/>
<layer number="95" name="Names" color="7" fill="1" visible="yes" active="yes"/>
<layer number="96" name="Values" color="7" fill="1" visible="yes" active="yes"/>
<layer number="97" name="Info" color="7" fill="1" visible="yes" active="yes"/>
<layer number="98" name="Guide" color="6" fill="1" visible="yes" active="yes"/>
<layer number="100" name="Muster" color="7" fill="1" visible="no" active="no"/>
<layer number="101" name="Patch_Top" color="12" fill="4" visible="yes" active="yes"/>
<layer number="102" name="Vscore" color="7" fill="1" visible="yes" active="yes"/>
<layer number="104" name="Name" color="7" fill="1" visible="yes" active="yes"/>
<layer number="116" name="Patch_BOT" color="9" fill="4" visible="yes" active="yes"/>
<layer number="121" name="_tsilk" color="7" fill="1" visible="yes" active="yes"/>
<layer number="122" name="_bsilk" color="7" fill="1" visible="yes" active="yes"/>
<layer number="151" name="HeatSink" color="7" fill="1" visible="yes" active="yes"/>
<layer number="200" name="200bmp" color="1" fill="10" visible="no" active="no"/>
<layer number="201" name="201bmp" color="2" fill="1" visible="no" active="no"/>
<layer number="202" name="202bmp" color="3" fill="1" visible="no" active="no"/>
<layer number="250" name="Descript" color="3" fill="1" visible="no" active="no"/>
<layer number="251" name="SMDround" color="12" fill="11" visible="no" active="no"/>
<layer number="254" name="cooling" color="7" fill="1" visible="yes" active="yes"/>
</layers>
<library>
<description>Bluetooth HC05 Module. See http://mcuoneclipse.com/2013/02/14/bluetooth-with-the-freedom-board/</description>
<packages>
<package name="BLUETOOTH_SMD">
<description>HC-05</description>
<wire x1="-6.35" y1="4.81" x2="-6.35" y2="13.31" width="0.127" layer="21"/>
<wire x1="-6.35" y1="13.31" x2="6.65" y2="13.31" width="0.127" layer="21"/>
<wire x1="6.65" y1="13.31" x2="6.65" y2="4.81" width="0.127" layer="21"/>
<smd name="1" x="-6.35" y="3.81" dx="2" dy="1" layer="1"/>
<smd name="2" x="-6.35" y="2.31" dx="2" dy="1" layer="1"/>
<smd name="3" x="-6.35" y="0.81" dx="2" dy="1" layer="1"/>
<smd name="4" x="-6.35" y="-0.69" dx="2" dy="1" layer="1"/>
<smd name="5" x="-6.35" y="-2.19" dx="2" dy="1" layer="1"/>
<smd name="6" x="-6.35" y="-3.69" dx="2" dy="1" layer="1"/>
<smd name="7" x="-6.35" y="-5.19" dx="2" dy="1" layer="1"/>
<smd name="8" x="-6.35" y="-6.69" dx="2" dy="1" layer="1"/>
<smd name="9" x="-6.35" y="-8.19" dx="2" dy="1" layer="1"/>
<smd name="10" x="-6.35" y="-9.69" dx="2" dy="1" layer="1"/>
<smd name="11" x="-6.35" y="-11.19" dx="2" dy="1" layer="1"/>
<smd name="12" x="-6.35" y="-12.69" dx="2" dy="1" layer="1"/>
<smd name="13" x="-6.35" y="-14.19" dx="2" dy="1" layer="1"/>
<smd name="22" x="6.65" y="-14.19" dx="2" dy="1" layer="1"/>
<smd name="23" x="6.65" y="-12.69" dx="2" dy="1" layer="1"/>
<smd name="24" x="6.65" y="-11.19" dx="2" dy="1" layer="1"/>
<smd name="25" x="6.65" y="-9.69" dx="2" dy="1" layer="1"/>
<smd name="26" x="6.65" y="-8.19" dx="2" dy="1" layer="1"/>
<smd name="27" x="6.65" y="-6.69" dx="2" dy="1" layer="1"/>
<smd name="28" x="6.65" y="-5.19" dx="2" dy="1" layer="1"/>
<smd name="29" x="6.65" y="-3.69" dx="2" dy="1" layer="1"/>
<smd name="30" x="6.65" y="-2.19" dx="2" dy="1" layer="1"/>
<smd name="31" x="6.65" y="-0.69" dx="2" dy="1" layer="1"/>
<smd name="32" x="6.65" y="0.81" dx="2" dy="1" layer="1"/>
<smd name="33" x="6.65" y="2.31" dx="2" dy="1" layer="1"/>
<smd name="34" x="6.65" y="3.81" dx="2" dy="1" layer="1"/>
<smd name="14" x="-5.1" y="-15.94" dx="1.8" dy="1" layer="1" rot="R90"/>
<smd name="15" x="-3.6" y="-15.94" dx="1.8" dy="1" layer="1" rot="R90"/>
<smd name="16" x="-2.1" y="-15.94" dx="1.8" dy="1" layer="1" rot="R90"/>
<smd name="17" x="-0.6" y="-15.94" dx="1.8" dy="1" layer="1" rot="R90"/>
<smd name="18" x="0.9" y="-15.94" dx="1.8" dy="1" layer="1" rot="R90"/>
<smd name="19" x="2.4" y="-15.94" dx="1.8" dy="1" layer="1" rot="R90"/>
<smd name="20" x="3.9" y="-15.94" dx="1.8" dy="1" layer="1" rot="R90"/>
<smd name="21" x="5.4" y="-15.94" dx="1.8" dy="1" layer="1" rot="R90"/>
<text x="-5.35" y="11.31" size="1.27" layer="25">&gt;name</text>
</package>
<package name="BT_BOARD_FOOTPRINT">
<description>Bluetooth Board V1.05 Footprint</description>
<pad name="RX" x="-16.51" y="3.81" drill="0.9" diameter="1.778"/>
<pad name="TX" x="-16.51" y="1.27" drill="0.9" diameter="1.778"/>
<pad name="GND" x="-16.51" y="-1.27" drill="0.9" diameter="1.778"/>
<text x="-15.24" y="3.556" size="0.6096" layer="21" font="vector">RX</text>
<text x="-15.24" y="1.016" size="0.6096" layer="21" font="vector">TX</text>
<text x="-15.24" y="-1.524" size="0.6096" layer="21" font="vector">GND</text>
<pad name="VCC" x="-16.51" y="-3.81" drill="0.9" diameter="1.778"/>
<text x="-15.24" y="-4.064" size="0.6096" layer="21" font="vector">VCC</text>
<wire x1="-17.78" y1="6.985" x2="-17.78" y2="-6.985" width="0.127" layer="21"/>
<wire x1="-17.78" y1="-6.985" x2="16.51" y2="-6.985" width="0.127" layer="21"/>
<wire x1="16.51" y1="-6.985" x2="16.51" y2="6.985" width="0.127" layer="21"/>
<wire x1="16.51" y1="6.985" x2="-17.78" y2="6.985" width="0.127" layer="21"/>
<text x="-17.78" y="7.493" size="1.016" layer="25" font="vector" ratio="12">&gt;NAME</text>
</package>
<package name="BT_BOARD_FOOTPRINT_STANDING">
<pad name="RX" x="-3.81" y="3.81" drill="0.9" diameter="1.6764"/>
<pad name="TX" x="-3.81" y="1.27" drill="0.9" diameter="1.6764"/>
<pad name="GND" x="-3.81" y="-1.27" drill="0.9" diameter="1.6764" shape="square"/>
<text x="-2.286" y="3.556" size="0.6096" layer="21" font="vector">RX</text>
<text x="-2.286" y="1.016" size="0.6096" layer="21" font="vector">TX</text>
<text x="-2.286" y="-1.524" size="0.6096" layer="21" font="vector">GND</text>
<pad name="VCC" x="-3.81" y="-3.81" drill="0.9" diameter="1.6764"/>
<text x="-2.286" y="-4.064" size="0.6096" layer="21" font="vector">VCC</text>
<wire x1="-2.48" y1="-7.985" x2="0.47" y2="-7.985" width="0.127" layer="21"/>
<wire x1="0.47" y1="7.985" x2="-2.58" y2="7.985" width="0.127" layer="21"/>
<text x="-5.08" y="5.293" size="0.8128" layer="25" font="vector" ratio="12">&gt;NAME</text>
<wire x1="-5.08" y1="-5.08" x2="-5.08" y2="5.08" width="0.127" layer="21"/>
<wire x1="-5.08" y1="5.08" x2="-2.54" y2="5.08" width="0.127" layer="21"/>
<wire x1="-2.54" y1="5.08" x2="-2.54" y2="7.95" width="0.127" layer="21"/>
<wire x1="-5.08" y1="-5.08" x2="-2.54" y2="-5.08" width="0.127" layer="21"/>
<wire x1="-2.54" y1="-5.08" x2="-2.54" y2="-7.95" width="0.127" layer="21"/>
</package>
</packages>
<symbols>
<symbol name="HC-05">
<wire x1="-17.78" y1="17.78" x2="-17.78" y2="-17.78" width="0.254" layer="94"/>
<wire x1="-17.78" y1="-17.78" x2="20.32" y2="-17.78" width="0.254" layer="94"/>
<wire x1="20.32" y1="-17.78" x2="20.32" y2="17.78" width="0.254" layer="94"/>
<wire x1="20.32" y1="17.78" x2="-17.78" y2="17.78" width="0.254" layer="94"/>
<text x="-17.78" y="22.86" size="1.778" layer="95">&gt;NAME</text>
<text x="-17.78" y="20.32" size="1.778" layer="96">&gt;VALUE</text>
<pin name="TX" x="-22.86" y="15.24" length="middle"/>
<pin name="RX" x="-22.86" y="12.7" length="middle"/>
<pin name="CTS" x="-22.86" y="10.16" length="middle"/>
<pin name="RTS" x="-22.86" y="7.62" length="middle"/>
<pin name="PCM_CLK" x="-22.86" y="5.08" length="middle"/>
<pin name="PCM_OUT" x="-22.86" y="2.54" length="middle"/>
<pin name="PCM_IN" x="-22.86" y="0" length="middle"/>
<pin name="PCN_SYNC" x="-22.86" y="-2.54" length="middle"/>
<pin name="AIO0" x="-22.86" y="-5.08" length="middle"/>
<pin name="AIO1" x="-22.86" y="-7.62" length="middle"/>
<pin name="RST" x="-22.86" y="-10.16" length="middle"/>
<pin name="3V3" x="-22.86" y="-12.7" length="middle"/>
<pin name="GND" x="-22.86" y="-15.24" length="middle"/>
<pin name="NC" x="-7.62" y="-22.86" length="middle" rot="R90"/>
<pin name="VBUSD-" x="-5.08" y="-22.86" length="middle" rot="R90"/>
<pin name="CSB" x="-2.54" y="-22.86" length="middle" rot="R90"/>
<pin name="MOSI" x="0" y="-22.86" length="middle" rot="R90"/>
<pin name="MISO" x="2.54" y="-22.86" length="middle" rot="R90"/>
<pin name="CLK" x="5.08" y="-22.86" length="middle" rot="R90"/>
<pin name="VBUSD+" x="7.62" y="-22.86" length="middle" rot="R90"/>
<pin name="GND1" x="10.16" y="-22.86" length="middle" rot="R90"/>
<pin name="GND2" x="25.4" y="-15.24" length="middle" rot="R180"/>
<pin name="PIO0" x="25.4" y="-12.7" length="middle" rot="R180"/>
<pin name="PIO1" x="25.4" y="-10.16" length="middle" rot="R180"/>
<pin name="PIO2" x="25.4" y="-7.62" length="middle" rot="R180"/>
<pin name="PIO3" x="25.4" y="-5.08" length="middle" rot="R180"/>
<pin name="PIO4" x="25.4" y="-2.54" length="middle" rot="R180"/>
<pin name="PIO5" x="25.4" y="0" length="middle" rot="R180"/>
<pin name="PIO6" x="25.4" y="2.54" length="middle" rot="R180"/>
<pin name="PIO7" x="25.4" y="5.08" length="middle" rot="R180"/>
<pin name="PIO8" x="25.4" y="7.62" length="middle" rot="R180"/>
<pin name="PIO9" x="25.4" y="10.16" length="middle" rot="R180"/>
<pin name="PIO10" x="25.4" y="12.7" length="middle" rot="R180"/>
<pin name="PIO11" x="25.4" y="15.24" length="middle" rot="R180"/>
</symbol>
<symbol name="BT_BOARD_SCHEMATIC">
<description>Bluetooth Board V1.05 Schematic</description>
<pin name="GND" x="-12.7" y="2.54" length="middle"/>
<pin name="VCC" x="-12.7" y="7.62" length="middle"/>
<pin name="TX" x="-12.7" y="-2.54" length="middle"/>
<pin name="RX" x="-12.7" y="-7.62" length="middle"/>
<wire x1="-7.62" y1="10.16" x2="-7.62" y2="-10.16" width="0.254" layer="94"/>
<wire x1="-7.62" y1="-10.16" x2="7.62" y2="-10.16" width="0.254" layer="94"/>
<wire x1="7.62" y1="-10.16" x2="7.62" y2="10.16" width="0.254" layer="94"/>
<wire x1="7.62" y1="10.16" x2="-7.62" y2="10.16" width="0.254" layer="94"/>
<text x="-7.62" y="10.922" size="1.778" layer="95" ratio="15">&gt;NAME</text>
<text x="-7.62" y="-12.7" size="1.778" layer="96" ratio="15">&gt;VALUE</text>
</symbol>
</symbols>
<devicesets>
<deviceset name="HC_05" prefix="U">
<description>HC-05 Bluetooth Module</description>
<gates>
<gate name="G$1" symbol="HC-05" x="0" y="0"/>
</gates>
<devices>
<device name="" package="BLUETOOTH_SMD">
<connects>
<connect gate="G$1" pin="3V3" pad="12"/>
<connect gate="G$1" pin="AIO0" pad="9"/>
<connect gate="G$1" pin="AIO1" pad="10"/>
<connect gate="G$1" pin="CLK" pad="19"/>
<connect gate="G$1" pin="CSB" pad="16"/>
<connect gate="G$1" pin="CTS" pad="3"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="GND1" pad="21"/>
<connect gate="G$1" pin="GND2" pad="22"/>
<connect gate="G$1" pin="MISO" pad="18"/>
<connect gate="G$1" pin="MOSI" pad="17"/>
<connect gate="G$1" pin="NC" pad="14"/>
<connect gate="G$1" pin="PCM_CLK" pad="5"/>
<connect gate="G$1" pin="PCM_IN" pad="7"/>
<connect gate="G$1" pin="PCM_OUT" pad="6"/>
<connect gate="G$1" pin="PCN_SYNC" pad="8"/>
<connect gate="G$1" pin="PIO0" pad="23"/>
<connect gate="G$1" pin="PIO1" pad="24"/>
<connect gate="G$1" pin="PIO10" pad="33"/>
<connect gate="G$1" pin="PIO11" pad="34"/>
<connect gate="G$1" pin="PIO2" pad="25"/>
<connect gate="G$1" pin="PIO3" pad="26"/>
<connect gate="G$1" pin="PIO4" pad="27"/>
<connect gate="G$1" pin="PIO5" pad="28"/>
<connect gate="G$1" pin="PIO6" pad="29"/>
<connect gate="G$1" pin="PIO7" pad="30"/>
<connect gate="G$1" pin="PIO8" pad="31"/>
<connect gate="G$1" pin="PIO9" pad="32"/>
<connect gate="G$1" pin="RST" pad="11"/>
<connect gate="G$1" pin="RTS" pad="4"/>
<connect gate="G$1" pin="RX" pad="2"/>
<connect gate="G$1" pin="TX" pad="1"/>
<connect gate="G$1" pin="VBUSD+" pad="20"/>
<connect gate="G$1" pin="VBUSD-" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BLUETOOTH_BOARD" prefix="J_BT_BOARD_">
<description>Bluetooth Board V1.05</description>
<gates>
<gate name="J_BT_BOARD" symbol="BT_BOARD_SCHEMATIC" x="0" y="0"/>
</gates>
<devices>
<device name="" package="BT_BOARD_FOOTPRINT">
<connects>
<connect gate="J_BT_BOARD" pin="GND" pad="GND"/>
<connect gate="J_BT_BOARD" pin="RX" pad="RX"/>
<connect gate="J_BT_BOARD" pin="TX" pad="TX"/>
<connect gate="J_BT_BOARD" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="STANDING" package="BT_BOARD_FOOTPRINT_STANDING">
<connects>
<connect gate="J_BT_BOARD" pin="GND" pad="GND"/>
<connect gate="J_BT_BOARD" pin="RX" pad="RX"/>
<connect gate="J_BT_BOARD" pin="TX" pad="TX"/>
<connect gate="J_BT_BOARD" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
